**Emergency Shower Blue Eagle UK309**

**(Instruction Book)**

**\*Usage**

This unit is not only the essential equipment of labor protection,but also the essential facilities against poisonous and corrosive material.If accidents happens,reduce the damage to the minimum degree by quickly spraying or washing the hurt.

**\*Main material**

Good quality stainless steel, shower head is made of stainless steel.

**\*Structure features**

Stainless steel ball valve switch, using conveniently, safety seal, use life is longer.

**\*Main function parameters**

|  |  |  |
| --- | --- | --- |
| Pressure | Flux L/Min | Temperature |
| Nominal pressure | Seal pressure | Working pressure | Shower | Tepid water |
| 0.4 | 0.45 | 0.20-0.40 | ≥75.5 |

Choosing these data is considering the hurt to the skin, eye(s), when accidents happen.

**\*Method of application**

Downward pull switch to open (angle 90),push up swith to close.

**\*Packing list**

|  |  |  |
| --- | --- | --- |
| **No.** | **Part name** | **Quanlity** |
| 1 | Shower head | 1 PCS |
| 2 | Shower switch handle | 1 PCS |
| 3 | Stainless steel pipe | 1 PCS |

